## Name

eaglectrl — advanced controls for eagle-usb driver.

## Synopsis

`eaglectrl` [`-h`|`--help`] [`-v`|`--version`] [`-o`|`--options `options-file``] [`-c`|`--cmvs `file``] [`-d`|`--dsp `dsp-file``] [`-i`|`--if`] [`-s`|`--sync `sec``] [`-p`|`--print`] [`-w`|`--wizard`] [`-g`|`--get-debug`] [`-x`|`--set-debug `debug-mask``] [`-l`|`--list-debug`]

## DESCRIPTION

This manual page documents briefly the eaglectrl commands.

## OPTIONS

`-h`, `--help`

  Show summary of options.

`-v`, `--version`

  Show the version number of program.

`-o`, `--options `file``

  Set options file (file defaults to /etc/eagle-usb/eagle-usb.conf).

`-c`, `--cmvs `file``

  Set cmvs file (file defaults to /etc/eagle-usb/CMVep.txt).

`-d`, `--dsp `dsp-file``

  Send Options, CMVS, and DSP file path is either a path to the DSP file or to a directory containing DSP files for ISDN and POTS. In this case eaglectrl will choose which file to send to modem depending on the modem type. Defaults to /usr/lib/eagle-usb.

`-i`, `--if`

  Print modem interface name.

`-s`, `--sync `sec``

  Wait `sec` seconds for modem to be operationnal. If sec is 0 wait until synchro happens (infinite). Defaults to 60.

`-p`, `--print`

  Display detected devices.

`-w`, `--wizard`

  Wizard mode. Works if you have ONLY 1 eagle modem plugged in. Choose itself sequence to send to modem (firmware/DSP ..) NOTE: You can use it in conjunction with -o, -d and -s to specify the options file, DSP file and synchro timeout values to use.

`-g`, `--get-debug`

  Get debug mask.

`-x`, `--set-debug `debug-mask``

  Set driver debug-mask to the given value, which can either be an haxadecimal number (0x0, 0xFF) or a list of debug flags separated by a comma. A list of available flags can be given by the `--list-debug` option.

`-l`, `--list-debug`

  Display a list of available flags for the debug-mask.

## SEE ALSO

eaglestat(8), eagleconfig(8), eaglediag(8), startadsl(8), stopadsl(8).