## Name

startadsl — start your eagle-usb dsl connection.

## Synopsis

`startadsl` [`-h`|`--help`] [`-m`|`--mire`] [`-s`|`--simple`] [`-t`|`--timeout=`sec``] [`-a`|`--ip=`x.x.x.x``] [`-d`|`--debug`]

## DESCRIPTION

startadsl start your eagle-usb dsl connection to Internet.

## OPTIONS

`-h`, `--help`

  Show summary of options.

`-m`, `--mire`

  Connect to the mire.

`-s`, `--simple`

  Use ifconfig instead of ifup/ifdown.

`-t`, `--timeout=`sec``

  Define delay for the modem to become operational.

`-a`xxx.xxx.xxx.xxx``, `--ip=`xxx.xxx.xxx.xxx``

  Use ip address, imply simple mode.

`-d`, `--debug`

  Launch pppd in debug mode.

## SEE ALSO

stopadsl(8), eaglectrl(8), eagleconfig(8).